Indexed mode of addressing

0(SP) - add 0 to Stack Pointer address

2(SP) - add 2 to Stack Pointer address

-2(SP) - add -2 to Stack Pointer address

etc.

stack pointer is changed after returning from subroutine